Next: Invoking, Previous: Top, Up: Top

## 1 Overview

Here is a brief summary of how to invoke `as`. For details, see Command-Line Options.

         as [-a[cdghlns][=file]] [--alternate] [-D]
          [--compress-debug-sections]  [--nocompress-debug-sections]
          [--debug-prefix-map old=new]
          [--defsym sym=val] [-f] [-g] [--gstabs]
          [--gstabs+] [--gdwarf-2] [--help] [-I dir] [-J]
          [-K] [-L] [--listing-lhs-width=NUM]
          [--listing-lhs-width2=NUM] [--listing-rhs-width=NUM]
          [--listing-cont-lines=NUM] [--keep-locals] [-o
          objfile] [-R] [--reduce-memory-overheads] [--statistics]
          [-v] [-version] [--version] [-W] [--warn]
          [--fatal-warnings] [-w] [-x] [-Z] [@FILE]
          [--target-help] [target-options]
          [--|files ...]

         Target Alpha options:
            [-mcpu]
            [-mdebug | -no-mdebug]
            [-replace | -noreplace]
            [-relax] [-g] [-Gsize]
            [-F] [-32addr]

         Target ARC options:
            [-marc[5|6|7|8]]
            [-EB|-EL]

         Target ARM options:

            [-mcpu=processor[+extension...]]
            [-march=architecture[+extension...]]
            [-mfpu=floating-point-format]
            [-mfloat-abi=abi]
            [-meabi=ver]
            [-mthumb]
            [-EB|-EL]
            [-mapcs-32|-mapcs-26|-mapcs-float|
             -mapcs-reentrant]
            [-mthumb-interwork] [-k]

         Target Blackfin options:
            [-mcpu=processor[-sirevision]]
            [-mfdpic]
            [-mno-fdpic]
            [-mnopic]

         Target CRIS options:
            [--underscore | --no-underscore]
            [--pic] [-N]
            [--emulation=criself | --emulation=crisaout]
            [--march=v0_v10 | --march=v10 | --march=v32 | --march=common_v10_v32]

         Target D10V options:
            [-O]

         Target D30V options:
            [-O|-n|-N]

         Target H8/300 options:
            [-h-tick-hex]

         Target i386 options:
            [--32|--64] [-n]
            [-march=CPU[+EXTENSION...]] [-mtune=CPU]

         Target i960 options:

            [-ACA|-ACA_A|-ACB|-ACC|-AKA|-AKB|
             -AKC|-AMC]
            [-b] [-no-relax]

         Target IA-64 options:
            [-mconstant-gp|-mauto-pic]
            [-milp32|-milp64|-mlp64|-mp64]
            [-mle|mbe]
            [-mtune=itanium1|-mtune=itanium2]
            [-munwind-check=warning|-munwind-check=error]
            [-mhint.b=ok|-mhint.b=warning|-mhint.b=error]
            [-x|-xexplicit] [-xauto] [-xdebug]

         Target IP2K options:
            [-mip2022|-mip2022ext]

         Target M32C options:
            [-m32c|-m16c] [-relax] [-h-tick-hex]

         Target M32R options:
            [--m32rx|--[no-]warn-explicit-parallel-conflicts|
            --W[n]p]

         Target M680X0 options:
            [-l] [-m68000|-m68010|-m68020|...]

         Target M68HC11 options:
            [-m68hc11|-m68hc12|-m68hcs12]
            [-mshort|-mlong]
            [-mshort-double|-mlong-double]
            [--force-long-branches] [--short-branches]
            [--strict-direct-mode] [--print-insn-syntax]
            [--print-opcodes] [--generate-example]

         Target MCORE options:
            [-jsri2bsr] [-sifilter] [-relax]
            [-mcpu=[210|340]]
         Target MICROBLAZE options:

         Target MIPS options:
            [-nocpp] [-EL] [-EB] [-O[optimization level]]
            [-g[debug level]] [-G num] [-KPIC] [-call_shared]
            [-non_shared] [-xgot [-mvxworks-pic]
            [-mabi=ABI] [-32] [-n32] [-64] [-mfp32] [-mgp32]
            [-march=CPU] [-mtune=CPU] [-mips1] [-mips2]
            [-mips3] [-mips4] [-mips5] [-mips32] [-mips32r2]
            [-mips64] [-mips64r2]
            [-construct-floats] [-no-construct-floats]
            [-trap] [-no-break] [-break] [-no-trap]
            [-mips16] [-no-mips16]
            [-msmartmips] [-mno-smartmips]
            [-mips3d] [-no-mips3d]
            [-mdmx] [-no-mdmx]
            [-mdsp] [-mno-dsp]
            [-mdspr2] [-mno-dspr2]
            [-mmt] [-mno-mt]
            [-mfix7000] [-mno-fix7000]
            [-mfix-vr4120] [-mno-fix-vr4120]
            [-mfix-vr4130] [-mno-fix-vr4130]
            [-mdebug] [-no-mdebug]
            [-mpdr] [-mno-pdr]

         Target MMIX options:
            [--fixed-special-register-names] [--globalize-symbols]
            [--gnu-syntax] [--relax] [--no-predefined-symbols]
            [--no-expand] [--no-merge-gregs] [-x]
            [--linker-allocated-gregs]

         Target PDP11 options:
            [-mpic|-mno-pic] [-mall] [-mno-extensions]
            [-mextension|-mno-extension]
            [-mcpu] [-mmachine]

         Target picoJava options:
            [-mb|-me]

         Target PowerPC options:
            [-mpwrx|-mpwr2|-mpwr|-m601|-mppc|-mppc32|-m603|-m604|
             -m403|-m405|-mppc64|-m620|-mppc64bridge|-mbooke]
            [-mcom|-many|-maltivec|-mvsx] [-memb]
            [-mregnames|-mno-regnames]
            [-mrelocatable|-mrelocatable-lib]
            [-mlittle|-mlittle-endian|-mbig|-mbig-endian]
            [-msolaris|-mno-solaris]

         Target RX options:
            [-mlittle-endian|-mbig-endian]
            [-m32bit-ints|-m16bit-ints]
            [-m32bit-doubles|-m64bit-doubles]

         Target s390 options:
            [-m31|-m64] [-mesa|-mzarch] [-march=CPU]
            [-mregnames|-mno-regnames]
            [-mwarn-areg-zero]

         Target SCORE options:
            [-EB][-EL][-FIXDD][-NWARN]
            [-SCORE5][-SCORE5U][-SCORE7][-SCORE3]
            [-march=score7][-march=score3]
            [-USE_R1][-KPIC][-O0][-G num][-V]

         Target SPARC options:

            [-Av6|-Av7|-Av8|-Asparclet|-Asparclite
             -Av8plus|-Av8plusa|-Av9|-Av9a]
            [-xarch=v8plus|-xarch=v8plusa] [-bump]
            [-32|-64]

         Target TIC54X options:
          [-mcpu=54[123589]|-mcpu=54[56]lp] [-mfar-mode|-mf]
          [-merrors-to-file <filename>|-me <filename>]

         Target TIC6X options:
            [-march=arch] [-matomic|-mno-atomic]
            [-mbig-endian|-mlittle-endian] [-mdsbt|-mno-dsbt]
            [-mpid=no|-mpid=near|-mpid=far] [-mpic|-mno-pic]

         Target Z80 options:
           [-z80] [-r800]
           [ -ignore-undocumented-instructions] [-Wnud]
           [ -ignore-unportable-instructions] [-Wnup]
           [ -warn-undocumented-instructions] [-Wud]
           [ -warn-unportable-instructions] [-Wup]
           [ -forbid-undocumented-instructions] [-Fud]
           [ -forbid-unportable-instructions] [-Fup]

         Target Xtensa options:
          [--[no-]text-section-literals] [--[no-]absolute-literals]
          [--[no-]target-align] [--[no-]longcalls]
          [--[no-]transform]
          [--rename-section oldname=newname]

`@`file
  Read command-line options from file. The options read are inserted in place of the original @file option. If file does not exist, or cannot be read, then the option will be treated literally, and not removed.

  Options in file are separated by whitespace. A whitespace character may be included in an option by surrounding the entire option in either single or double quotes. Any character (including a backslash) may be included by prefixing the character to be included with a backslash. The file may itself contain additional @file options; any such options will be processed recursively.

`-a[cdghlmns]`
  Turn on listings, in any of a variety of ways:
  `-ac`
    omit false conditionals
  `-ad`
    omit debugging directives
  `-ag`
    include general information, like as version and options passed
  `-ah`
    include high-level source
  `-al`
    include assembly
  `-am`
    include macro expansions
  `-an`
    omit forms processing
  `-as`
    include symbols
  `=file`
    set the name of the listing file

  You may combine these options; for example, use ‘`-aln`’ for assembly listing without forms processing. The ‘`=file`’ option, if used, must be the last one. By itself, ‘`-a`’ defaults to ‘`-ahls`’.

`--alternate`
  Begin in alternate macro mode. See `.altmacro`.
`--compress-debug-sections`
  Compress DWARF debug sections using zlib. The debug sections are renamed to begin with ‘`.zdebug`’, and the resulting object file may not be compatible with older linkers and object file utilities.
`--nocompress-debug-sections`
  Do not compress DWARF debug sections. This is the default.
`-D`
  Ignored. This option is accepted for script compatibility with calls to other assemblers.
`--debug-prefix-map` old`=`new
  When assembling files in directory `old`, record debugging information describing them as in `new` instead.
`--defsym` sym`=`value
  Define the symbol sym to be value before assembling the input file. value must be an integer constant. As in C, a leading ‘`0x`’ indicates a hexadecimal value, and a leading ‘`0`’ indicates an octal value. The value of the symbol can be overridden inside a source file via the use of a `.set` pseudo-op.
`-f`
  “fast”—skip whitespace and comment preprocessing (assume source is compiler output).
`-g`
`--gen-debug`
  Generate debugging information for each assembler source line using whichever debug format is preferred by the target. This currently means either STABS, ECOFF or DWARF2.
`--gstabs`
  Generate stabs debugging information for each assembler line. This may help debugging assembler code, if the debugger can handle it.
`--gstabs+`
  Generate stabs debugging information for each assembler line, with GNU extensions that probably only gdb can handle, and that could make other debuggers crash or refuse to read your program. This may help debugging assembler code. Currently the only GNU extension is the location of the current working directory at assembling time.
`--gdwarf-2`
  Generate DWARF2 debugging information for each assembler line. This may help debugging assembler code, if the debugger can handle it. Note—this option is only supported by some targets, not all of them.
`--help`
  Print a summary of the command line options and exit.
`--target-help`
  Print a summary of all target specific options and exit.
`-I` dir
  Add directory dir to the search list for `.include` directives.
`-J`
  Don't warn about signed overflow.
`-K`
  Issue warnings when difference tables altered for long displacements.
`-L`
`--keep-locals`
  Keep (in the symbol table) local symbols. These symbols start with system-specific local label prefixes, typically ‘`.L`’ for ELF systems or ‘`L`’ for traditional a.out systems. See Symbol Names.
`--listing-lhs-width=`number
  Set the maximum width, in words, of the output data column for an assembler listing to number.
`--listing-lhs-width2=`number
  Set the maximum width, in words, of the output data column for continuation lines in an assembler listing to number.
`--listing-rhs-width=`number
  Set the maximum width of an input source line, as displayed in a listing, to number bytes.
`--listing-cont-lines=`number
  Set the maximum number of lines printed in a listing for a single line of input to number + 1.
`-o` objfile
  Name the object-file output from `as` objfile.
`-R`
  Fold the data section into the text section.

  Set the default size of GAS's hash tables to a prime number close to number. Increasing this value can reduce the length of time it takes the assembler to perform its tasks, at the expense of increasing the assembler's memory requirements. Similarly reducing this value can reduce the memory requirements at the expense of speed.

`--reduce-memory-overheads`
  This option reduces GAS's memory requirements, at the expense of making the assembly processes slower. Currently this switch is a synonym for ‘`--hash-size=4051`’, but in the future it may have other effects as well.
`--statistics`
  Print the maximum space (in bytes) and total time (in seconds) used by assembly.
`--strip-local-absolute`
  Remove local absolute symbols from the outgoing symbol table.
`-v`
`-version`
  Print the `as` version.
`--version`
  Print the `as` version and exit.
`-W`
`--no-warn`
  Suppress warning messages.
`--fatal-warnings`
  Treat warnings as errors.
`--warn`
  Don't suppress warning messages or treat them as errors.
`-w`
  Ignored.
`-x`
  Ignored.
`-Z`
  Generate an object file even after errors.
`-- |` files`...`
  Standard input, or source files to assemble.

The following options are available when as is configured for an ARC processor.

`-marc[5|6|7|8]`
  This option selects the core processor variant.
`-EB | -EL`
  Select either big-endian (-EB) or little-endian (-EL) output.

The following options are available when as is configured for the ARM processor family.

`-mcpu=`processor`[+`extension`...]`
  Specify which ARM processor variant is the target.
`-march=`architecture`[+`extension`...]`
  Specify which ARM architecture variant is used by the target.
`-mfpu=`floating-point-format
  Select which Floating Point architecture is the target.
`-mfloat-abi=`abi
  Select which floating point ABI is in use.
`-mthumb`
  Enable Thumb only instruction decoding.
`-mapcs-32 | -mapcs-26 | -mapcs-float | -mapcs-reentrant`
  Select which procedure calling convention is in use.
`-EB | -EL`
  Select either big-endian (-EB) or little-endian (-EL) output.
`-mthumb-interwork`
  Specify that the code has been generated with interworking between Thumb and ARM code in mind.
`-k`
  Specify that PIC code has been generated.

The following options are available when as is configured for the Blackfin processor family.

`-mcpu=`processor[`-`sirevision]
  This option specifies the target processor. The optional sirevision is not used in assembler.
`-mfdpic`
  Assemble for the FDPIC ABI.
`-mno-fdpic`
`-mnopic`
  Disable -mfdpic.

See the info pages for documentation of the CRIS-specific options.

The following options are available when as is configured for a D10V processor.

`-O`
  Optimize output by parallelizing instructions.

The following options are available when as is configured for a D30V processor.

`-O`
  Optimize output by parallelizing instructions.

`-n`
  Warn when nops are generated.

`-N`
  Warn when a nop after a 32-bit multiply instruction is generated.

The following options are available when as is configured for the Intel 80960 processor.

`-ACA | -ACA_A | -ACB | -ACC | -AKA | -AKB | -AKC | -AMC`
  Specify which variant of the 960 architecture is the target.
`-b`
  Add code to collect statistics about branches taken.
`-no-relax`
  Do not alter compare-and-branch instructions for long displacements; error if necessary.

The following options are available when as is configured for the Ubicom IP2K series.

`-mip2022ext`
  Specifies that the extended IP2022 instructions are allowed.
`-mip2022`
  Restores the default behaviour, which restricts the permitted instructions to just the basic IP2022 ones.

The following options are available when as is configured for the Renesas M32C and M16C processors.

`-m32c`
  Assemble M32C instructions.
`-m16c`
  Assemble M16C instructions (the default).
`-relax`
  Enable support for link-time relaxations.
`-h-tick-hex`
  Support H'00 style hex constants in addition to 0x00 style.

The following options are available when as is configured for the Renesas M32R (formerly Mitsubishi M32R) series.

`--m32rx`
  Specify which processor in the M32R family is the target. The default is normally the M32R, but this option changes it to the M32RX.
`--warn-explicit-parallel-conflicts or --Wp`
  Produce warning messages when questionable parallel constructs are encountered.
`--no-warn-explicit-parallel-conflicts or --Wnp`
  Do not produce warning messages when questionable parallel constructs are encountered.

The following options are available when as is configured for the Motorola 68000 series.

`-l`
  Shorten references to undefined symbols, to one word instead of two.
`-m68000 | -m68008 | -m68010 | -m68020 | -m68030`
`| -m68040 | -m68060 | -m68302 | -m68331 | -m68332`
`| -m68333 | -m68340 | -mcpu32 | -m5200`
  Specify what processor in the 68000 family is the target. The default is normally the 68020, but this can be changed at configuration time.
`-m68881 | -m68882 | -mno-68881 | -mno-68882`
  The target machine does (or does not) have a floating-point coprocessor. The default is to assume a coprocessor for 68020, 68030, and cpu32. Although the basic 68000 is not compatible with the 68881, a combination of the two can be specified, since it's possible to do emulation of the coprocessor instructions with the main processor.
`-m68851 | -mno-68851`
  The target machine does (or does not) have a memory-management unit coprocessor. The default is to assume an MMU for 68020 and up.

For details about the PDP-11 machine dependent features options, see PDP-11-Options.

`-mpic | -mno-pic`
  Generate position-independent (or position-dependent) code. The default is `-mpic`.
`-mall`
`-mall-extensions`
  Enable all instruction set extensions. This is the default.
`-mno-extensions`
  Disable all instruction set extensions.
`-m` extension`| -mno-`extension
  Enable (or disable) a particular instruction set extension.
`-m` cpu
  Enable the instruction set extensions supported by a particular CPU, and disable all other extensions.
`-m` machine
  Enable the instruction set extensions supported by a particular machine model, and disable all other extensions.

The following options are available when as is configured for a picoJava processor.

`-mb`
  Generate “big endian” format output.

`-ml`
  Generate “little endian” format output.

The following options are available when as is configured for the Motorola 68HC11 or 68HC12 series.

`-m68hc11 | -m68hc12 | -m68hcs12`
  Specify what processor is the target. The default is defined by the configuration option when building the assembler.
`-mshort`
  Specify to use the 16-bit integer ABI.
`-mlong`
  Specify to use the 32-bit integer ABI.
`-mshort-double`
  Specify to use the 32-bit double ABI.
`-mlong-double`
  Specify to use the 64-bit double ABI.
`--force-long-branches`
  Relative branches are turned into absolute ones. This concerns conditional branches, unconditional branches and branches to a sub routine.
`-S | --short-branches`
  Do not turn relative branches into absolute ones when the offset is out of range.
`--strict-direct-mode`
  Do not turn the direct addressing mode into extended addressing mode when the instruction does not support direct addressing mode.
`--print-insn-syntax`
  Print the syntax of instruction in case of error.
`--print-opcodes`
  print the list of instructions with syntax and then exit.
`--generate-example`
  print an example of instruction for each possible instruction and then exit. This option is only useful for testing `as`.

The following options are available when `as` is configured for the SPARC architecture:

`-Av6 | -Av7 | -Av8 | -Asparclet | -Asparclite`
`-Av8plus | -Av8plusa | -Av9 | -Av9a`
  Explicitly select a variant of the SPARC architecture.

  ‘`-Av8plus`’ and ‘`-Av8plusa`’ select a 32 bit environment. ‘`-Av9`’ and ‘`-Av9a`’ select a 64 bit environment.

  ‘`-Av8plusa`’ and ‘`-Av9a`’ enable the SPARC V9 instruction set with UltraSPARC extensions.

`-xarch=v8plus | -xarch=v8plusa`
  For compatibility with the Solaris v9 assembler. These options are equivalent to -Av8plus and -Av8plusa, respectively.
`-bump`
  Warn when the assembler switches to another architecture.

The following options are available when as is configured for the 'c54x architecture.

`-mfar-mode`
  Enable extended addressing mode. All addresses and relocations will assume extended addressing (usually 23 bits).
`-mcpu=`CPU_VERSION
  Sets the CPU version being compiled for.
`-merrors-to-file` FILENAME
  Redirect error output to a file, for broken systems which don't support such behaviour in the shell.

The following options are available when as is configured for a mips processor.

`-G` num
  This option sets the largest size of an object that can be referenced implicitly with the `gp` register. It is only accepted for targets that use ECOFF format, such as a DECstation running Ultrix. The default value is 8.

`-EB`
  Generate “big endian” format output.

`-EL`
  Generate “little endian” format output.

`-mips1`
`-mips2`
`-mips3`
`-mips4`
`-mips5`
`-mips32`
`-mips32r2`
`-mips64`
`-mips64r2`
  Generate code for a particular mips Instruction Set Architecture level. ‘`-mips1`’ is an alias for ‘`-march=r3000`’, ‘`-mips2`’ is an alias for ‘`-march=r6000`’, ‘`-mips3`’ is an alias for ‘`-march=r4000`’ and ‘`-mips4`’ is an alias for ‘`-march=r8000`’. ‘`-mips5`’, ‘`-mips32`’, ‘`-mips32r2`’, ‘`-mips64`’, and ‘`-mips64r2`’ correspond to generic ‘`MIPS V`’, ‘`MIPS32`’, ‘`MIPS32 Release 2`’, ‘`MIPS64`’, and ‘`MIPS64 Release 2`’ ISA processors, respectively.
`-march=`CPU
  Generate code for a particular mips cpu.
`-mtune=`cpu
  Schedule and tune for a particular mips cpu.
`-mfix7000`
`-mno-fix7000`
  Cause nops to be inserted if the read of the destination register of an mfhi or mflo instruction occurs in the following two instructions.
`-mdebug`
`-no-mdebug`
  Cause stabs-style debugging output to go into an ECOFF-style .mdebug section instead of the standard ELF .stabs sections.
`-mpdr`
`-mno-pdr`
  Control generation of `.pdr` sections.
`-mgp32`
`-mfp32`
  The register sizes are normally inferred from the ISA and ABI, but these flags force a certain group of registers to be treated as 32 bits wide at all times. ‘`-mgp32`’ controls the size of general-purpose registers and ‘`-mfp32`’ controls the size of floating-point registers.
`-mips16`
`-no-mips16`
  Generate code for the MIPS 16 processor. This is equivalent to putting `.set mips16` at the start of the assembly file. ‘`-no-mips16`’ turns off this option.
`-msmartmips`
`-mno-smartmips`
  Enables the SmartMIPS extension to the MIPS32 instruction set. This is equivalent to putting `.set smartmips` at the start of the assembly file. ‘`-mno-smartmips`’ turns off this option.
`-mips3d`
`-no-mips3d`
  Generate code for the MIPS-3D Application Specific Extension. This tells the assembler to accept MIPS-3D instructions. ‘`-no-mips3d`’ turns off this option.
`-mdmx`
`-no-mdmx`
  Generate code for the MDMX Application Specific Extension. This tells the assembler to accept MDMX instructions. ‘`-no-mdmx`’ turns off this option.
`-mdsp`
`-mno-dsp`
  Generate code for the DSP Release 1 Application Specific Extension. This tells the assembler to accept DSP Release 1 instructions. ‘`-mno-dsp`’ turns off this option.
`-mdspr2`
`-mno-dspr2`
  Generate code for the DSP Release 2 Application Specific Extension. This option implies -mdsp. This tells the assembler to accept DSP Release 2 instructions. ‘`-mno-dspr2`’ turns off this option.
`-mmt`
`-mno-mt`
  Generate code for the MT Application Specific Extension. This tells the assembler to accept MT instructions. ‘`-mno-mt`’ turns off this option.
`--construct-floats`
`--no-construct-floats`
  The ‘`--no-construct-floats`’ option disables the construction of double width floating point constants by loading the two halves of the value into the two single width floating point registers that make up the double width register. By default ‘`--construct-floats`’ is selected, allowing construction of these floating point constants.

`--emulation=`name
  This option causes `as` to emulate `as` configured for some other target, in all respects, including output format (choosing between ELF and ECOFF only), handling of pseudo-opcodes which may generate debugging information or store symbol table information, and default endianness. The available configuration names are: ‘`mipsecoff`’, ‘`mipself`’, ‘`mipslecoff`’, ‘`mipsbecoff`’, ‘`mipslelf`’, ‘`mipsbelf`’. The first two do not alter the default endianness from that of the primary target for which the assembler was configured; the others change the default to little- or big-endian as indicated by the ‘`b`’ or ‘`l`’ in the name. Using ‘`-EB`’ or ‘`-EL`’ will override the endianness selection in any case.

  This option is currently supported only when the primary target `as` is configured for is a mips ELF or ECOFF target. Furthermore, the primary target or others specified with ‘`--enable-targets=...`’ at configuration time must include support for the other format, if both are to be available. For example, the Irix 5 configuration includes support for both.

  Eventually, this option will support more configurations, with more fine-grained control over the assembler's behavior, and will be supported for more processors.

`-nocpp`
  `as` ignores this option. It is accepted for compatibility with the native tools.
`--trap`
`--no-trap`
`--break`
`--no-break`
  Control how to deal with multiplication overflow and division by zero. ‘`--trap`’ or ‘`--no-break`’ (which are synonyms) take a trap exception (and only work for Instruction Set Architecture level 2 and higher); ‘`--break`’ or ‘`--no-trap`’ (also synonyms, and the default) take a break exception.
`-n`
  When this option is used, `as` will issue a warning every time it generates a nop instruction from a macro.

The following options are available when as is configured for an MCore processor.

`-jsri2bsr`
`-nojsri2bsr`
  Enable or disable the JSRI to BSR transformation. By default this is enabled. The command line option ‘`-nojsri2bsr`’ can be used to disable it.
`-sifilter`
`-nosifilter`
  Enable or disable the silicon filter behaviour. By default this is disabled. The default can be overridden by the ‘`-sifilter`’ command line option.
`-relax`
  Alter jump instructions for long displacements.
`-mcpu=[210|340]`
  Select the cpu type on the target hardware. This controls which instructions can be assembled.
`-EB`
  Assemble for a big endian target.
`-EL`
  Assemble for a little endian target.

See the info pages for documentation of the MMIX-specific options.

See the info pages for documentation of the RX-specific options.

The following options are available when as is configured for the s390 processor family.

`-m31`
`-m64`
  Select the word size, either 31/32 bits or 64 bits.
`-mesa`
`-mzarch`
  Select the architecture mode, either the Enterprise System Architecture (esa) or the z/Architecture mode (zarch).
`-march=`processor
  Specify which s390 processor variant is the target, ‘`g6`’, ‘`g6`’, ‘`z900`’, ‘`z990`’, ‘`z9-109`’, ‘`z9-ec`’, or ‘`z10`’.
`-mregnames`
`-mno-regnames`
  Allow or disallow symbolic names for registers.
`-mwarn-areg-zero`
  Warn whenever the operand for a base or index register has been specified but evaluates to zero.

The following options are available when as is configured for a TMS320C6000 processor.

`-march=`arch
  Enable (only) instructions from architecture arch. By default, all instructions are permitted.

  The following values of arch are accepted: `c62x`, `c64x`, `c64x+`, `c67x`, `c67x+`, `c674x`.

`-matomic`
`-mno-atomic`
  Enable or disable the optional C64x+ atomic operation instructions. By default, they are enabled if no `-march` option is given, or if an architecture is specified with `-march` that implies these instructions are present (currently, there are no such architectures); they are disabled if an architecture is specified with `-march` on which the instructions are optional or not present. This option overrides such a default from the architecture, independent of the order in which the `-march` or `-matomic` or `-mno-atomic` options are passed.
`-mdsbt`
`-mno-dsbt`
  The `-mdsbt` option causes the assembler to generate the `Tag_ABI_DSBT` attribute with a value of 1, indicating that the code is using DSBT addressing. The `-mno-dsbt` option, the default, causes the tag to have a value of 0, indicating that the code does not use DSBT addressing. The linker will emit a warning if objects of different type (DSBT and non-DSBT) are linked together.
`-mpid=no`
`-mpid=near`
`-mpid=far`
  The `-mpid=` option causes the assembler to generate the `Tag_ABI_PID` attribute with a value indicating the form of data addressing used by the code. `-mpid=no`, the default, indicates position-dependent data addressing, `-mpid=near` indicates position-independent addressing with GOT accesses using near DP addressing, and `-mpid=far` indicates position-independent addressing with GOT accesses using far DP addressing. The linker will emit a warning if objects built with different settings of this option are linked together.
`-mpic`
`-mno-pic`
  The `-mpic` option causes the assembler to generate the `Tag_ABI_PIC` attribute with a value of 1, indicating that the code is using position-independent code addressing, The `-mno-pic` option, the default, causes the tag to have a value of 0, indicating position-dependent code addressing. The linker will emit a warning if objects of different type (position-dependent and position-independent) are linked together.
`-mbig-endian`
`-mlittle-endian`
  Generate code for the specified endianness. The default is little-endian.

The following options are available when as is configured for an Xtensa processor.

`--text-section-literals | --no-text-section-literals`
  With `--text-section-literals`, literal pools are interspersed in the text section. The default is `--no-text-section-literals`, which places literals in a separate section in the output file. These options only affect literals referenced via PC-relative `L32R` instructions; literals for absolute mode `L32R` instructions are handled separately.
`--absolute-literals | --no-absolute-literals`
  Indicate to the assembler whether `L32R` instructions use absolute or PC-relative addressing. The default is to assume absolute addressing if the Xtensa processor includes the absolute `L32R` addressing option. Otherwise, only the PC-relative `L32R` mode can be used.
`--target-align | --no-target-align`
  Enable or disable automatic alignment to reduce branch penalties at the expense of some code density. The default is `--target-align`.
`--longcalls | --no-longcalls`
  Enable or disable transformation of call instructions to allow calls across a greater range of addresses. The default is `--no-longcalls`.
`--transform | --no-transform`
  Enable or disable all assembler transformations of Xtensa instructions. The default is `--transform`; `--no-transform` should be used only in the rare cases when the instructions must be exactly as specified in the assembly source.
`--rename-section` oldname`=`newname
  When generating output sections, rename the oldname section to newname.

The following options are available when as is configured for a Z80 family processor.

`-z80`
  Assemble for Z80 processor.
`-r800`
  Assemble for R800 processor.
`-ignore-undocumented-instructions`
`-Wnud`
  Assemble undocumented Z80 instructions that also work on R800 without warning.
`-ignore-unportable-instructions`
`-Wnup`
  Assemble all undocumented Z80 instructions without warning.
`-warn-undocumented-instructions`
`-Wud`
  Issue a warning for undocumented Z80 instructions that also work on R800.
`-warn-unportable-instructions`
`-Wup`
  Issue a warning for undocumented Z80 instructions that do not work on R800.
`-forbid-undocumented-instructions`
`-Fud`
  Treat all undocumented instructions as errors.
`-forbid-unportable-instructions`
`-Fup`
  Treat undocumented Z80 instructions that do not work on R800 as errors.