Previous: Xtensa Call Relaxation, Up: Xtensa Relaxation

##### 9.42.4.3 Other Immediate Field Relaxation

The assembler normally performs the following other relaxations. They can be disabled by using underscore prefixes (see Opcode Names), the ‘`--no-transform`’ command-line option (see Command Line Options), or the `no-transform` directive (see transform).

The `MOVI` machine instruction can only materialize values in the range from -2048 to 2047. Values outside this range are best materialized with `L32R` instructions. Thus:

             movi a0, 100000

is assembled into the following machine code:

             .literal .L1, 100000
             l32r a0, .L1

The `L8UI` machine instruction can only be used with immediate offsets in the range from 0 to 255. The `L16SI` and `L16UI` machine instructions can only be used with offsets from 0 to 510. The `L32I` machine instruction can only be used with offsets from 0 to 1020. A load offset outside these ranges can be materialized with an `L32R` instruction if the destination register of the load is different than the source address register. For example:

             l32i a1, a0, 2040

is translated to:

             .literal .L1, 2040
             l32r a1, .L1
             add a1, a0, a1
             l32i a1, a1, 0

If the load destination and source address register are the same, an out-of-range offset causes an error.

The Xtensa `ADDI` instruction only allows immediate operands in the range from -128 to 127. There are a number of alternate instruction sequences for the `ADDI` operation. First, if the immediate is 0, the `ADDI` will be turned into a `MOV.N` instruction (or the equivalent `OR` instruction if the code density option is not available). If the `ADDI` immediate is outside of the range -128 to 127, but inside the range -32896 to 32639, an `ADDMI` instruction or `ADDMI`/`ADDI` sequence will be used. Finally, if the immediate is outside of this range and a free register is available, an `L32R`/`ADD` sequence will be used with a literal allocated from the literal pool.

For example:

             addi    a5, a6, 0
             addi    a5, a6, 512
             addi    a5, a6, 513
             addi    a5, a6, 50000

is assembled into the following:

             .literal .L1, 50000
             mov.n   a5, a6
             addmi   a5, a6, 0x200
             addmi   a5, a6, 0x200
             addi    a5, a5, 1
             l32r    a5, .L1
             add     a5, a6, a5