Next: RL78-Directives, Previous: RL78-Opts, Up: RL78-Dependent [Contents][Index]

#### 9.35.2 Symbolic Operand Modifiers

The RL78 has three modifiers that adjust the relocations used by the linker:

`%lo16()`

  When loading a 20-bit (or wider) address into registers, this modifier selects the 16 least significant bits.

        movw ax,#%lo16(_sym)

`%hi16()`

  When loading a 20-bit (or wider) address into registers, this modifier selects the 16 most significant bits.

        movw ax,#%hi16(_sym)

`%hi8()`

  When loading a 20-bit (or wider) address into registers, this modifier selects the 8 bits that would go into CS or ES (i.e. bits 23..16).

        mov es, #%hi8(_sym)