Next: LM32 Options, Previous: IA-64 Options, Up: Submodel Options [Contents][Index]

#### 3.17.19 IA-64/VMS Options

These ‘`-m`’ options are defined for the IA-64/VMS implementations:

`-mvms-return-codes`

  Return VMS condition codes from main. The default is to return POSIX style condition (e.g. error) codes.

`-mdebug-main=prefix`

  Flag the first routine whose name starts with prefix as the main routine for the debugger.

`-mmalloc64`

  Default to 64-bit memory allocation routines.