Next: RX-Modifiers, Up: RX-Dependent [Contents][Index]

#### 9.36.1 RX Options

The Renesas RX port of `as` has a few target specfic command line options:

`-m32bit-doubles`

  This option controls the ABI and indicates to use a 32-bit float ABI. It has no effect on the assembled instructions, but it does influence the behaviour of the ‘`.double`’ pseudo-op. This is the default.

`-m64bit-doubles`

  This option controls the ABI and indicates to use a 64-bit float ABI. It has no effect on the assembled instructions, but it does influence the behaviour of the ‘`.double`’ pseudo-op.

`-mbig-endian`

  This option controls the ABI and indicates to use a big-endian data ABI. It has no effect on the assembled instructions, but it does influence the behaviour of the ‘`.short`’, ‘`.hword`’, ‘`.int`’, ‘`.word`’, ‘`.long`’, ‘`.quad`’ and ‘`.octa`’ pseudo-ops.

`-mlittle-endian`

  This option controls the ABI and indicates to use a little-endian data ABI. It has no effect on the assembled instructions, but it does influence the behaviour of the ‘`.short`’, ‘`.hword`’, ‘`.int`’, ‘`.word`’, ‘`.long`’, ‘`.quad`’ and ‘`.octa`’ pseudo-ops. This is the default.

`-muse-conventional-section-names`

  This option controls the default names given to the code (.text), initialised data (.data) and uninitialised data sections (.bss).

`-muse-renesas-section-names`

  This option controls the default names given to the code (.P), initialised data (.D_1) and uninitialised data sections (.B_1). This is the default.

`-msmall-data-limit`

  This option tells the assembler that the small data limit feature of the RX port of GCC is being used. This results in the assembler generating an undefined reference to a symbol called `__gp` for use by the relocations that are needed to support the small data limit feature. This option is not enabled by default as it would otherwise pollute the symbol table.

`-mpid`

  This option tells the assembler that the position independent data of the RX port of GCC is being used. This results in the assembler generating an undefined reference to a symbol called `__pid_base`, and also setting the RX_PID flag bit in the e_flags field of the ELF header of the object file.

`-mint-register=num`

  This option tells the assembler how many registers have been reserved for use by interrupt handlers. This is needed in order to compute the correct values for the `%gpreg` and `%pidreg` meta registers.

`-mgcc-abi`

  This option tells the assembler that the old GCC ABI is being used by the assembled code. With this version of the ABI function arguments that are passed on the stack are aligned to a 32-bit boundary.

`-mrx-abi`

  This option tells the assembler that the official RX ABI is being used by the assembled code. With this version of the ABI function arguments that are passed on the stack are aligned to their natural alignments. This option is the default.

`-mcpu=name`

  This option tells the assembler the target CPU type. Currently the `rx200`, `rx600` and `rx610` are recognised as valid cpu names. Attempting to assemble an instruction not supported by the indicated cpu type will result in an error message being generated.

Next: RX-Modifiers, Up: RX-Dependent [Contents][Index]