Next: MSP430 Opcodes, Previous: MSP430 Floating Point, Up: MSP430-Dependent [Contents][Index]

#### 9.29.4 MSP 430 Machine Directives

`.file`

  This directive is ignored; it is accepted for compatibility with other MSP 430 assemblers.

  > Warning: in other versions of the GNU assembler, `.file` is used for the directive called `.app-file` in the MSP 430 support.

`.line`

  This directive is ignored; it is accepted for compatibility with other MSP 430 assemblers.

`.arch`

  Sets the target microcontroller in the same way as the `-mmcu` command line option.

`.cpu`

  Sets the target architecture in the same way as the `-mcpu` command line option.

`.profiler`

  This directive instructs assembler to add new profile entry to the object file.