Next: RL78-Syntax, Previous: RL78-Modifiers, Up: RL78-Dependent [Contents][Index]

#### 9.35.3 Assembler Directives

In addition to the common directives, the RL78 adds these:

`.double`

  Output a constant in “double” format, which is a 32-bit floating point value on RL78.

`.bss`

  Select the BSS section.

`.3byte`

  Output a constant value in a three byte format.

`.int`
`.word`

  Output a constant value in a four byte format.